QUESTION:

Write an assembly language program for Multiplying two 8-bit data using 8086 processor.

PROGRAM:

lda 2001

mov b,a

lda 2005

mov c,a

mvi a,00h

loop: add b

dcr c

jnz loop

sta 2007

hlt

OUTPUT:

